|  |  |  |
| --- | --- | --- |
| **To:**  **Vaga Refrigeration**  **Nithin Nair** | **Quote: 13423**  **Tag: Door Order** | **From:** **Mr. Pabla** |
| **Tel: 1-437-808-9919** | **Email**: **nmn@vagainc.ca** | **Date: Sept 24**, 2024 |

**Flat Frame Doors**

**Cooler – 34” X 78” High - (Plywood Flat Frame $ 1080.00 x 8 = 8,640.00 + Tax**

**Freezer – 34” X 78” High - (Plywood Flat Frame $ 1130.00 x 2 = 2,260 + Tax**

***Quantity: 2 (abn24vr1)***

Freezer ABN Standard Solid Hinged Flat Frame Door **34” x 78” High**, Complete with Spring loaded Hinges, Latch, Strike, Inside Release Handle, Magnetic Gasket, Kick Plate, Door Closure, Door Sweep & Hardware**. 4” / Left Hand With 4” Floor**

***Quantity: 3 (abn24vr3)***

Cooler ABN Standard Solid Hinged Flat Frame Door **34” x 78” High**, Complete with Spring Loaded Hinges, Latch, Strike, Inside Release Handle, Magnetic Gasket, Kick Plate, Door Closure, Door Sweep & Hardware**. 4” / Left Hand No Floor**

***Quantity: 5 (abn24vr3)***

Cooler ABN Standard Solid Hinged Flat Frame Door **34” x 78” High**, Complete with Spring Loaded Hinges, Latch, Strike, Inside Release Handle, Magnetic Gasket, Kick Plate, Door Closure, Door Sweep & Hardware**. 4” / Right Hand No Floor**

***By Others: Electrical and Plumbing.***

**Terms & Conditions: *\*\*All applicable taxes extra\*\****

1. **Terms 30% deposit with P.O. Final payment must be received on delivery or at the time of pick up.**
2. Administration charge of 2.4% per month will be charged on all overdue accounts.
3. All goods remain the exclusive property of ABN Refrigeration Mfg. until payment in full is received. ABN Refrigeration Mfg. also reserves the right to remove the equipment from the location if failure to complete all financial transactions at any time without notice.
4. **Any Customer Changes Once Drawing is Approved Will Incur Extra Charges.**
5. **NOTE: “Delivery Is FOB ABN warehouse & IS QUOTED FOR GTA DELIVERY Unless Otherwise Stated IN THE QUOTE.”**
6. **Owners/Purchasers Responsibility**: to provide adequate ventilation for air cooled systems at the condensing unit location for proper operation, with maximum ambient temperature of 32.2 C/90F & min. of 10C/50F. The owner is responsible to ensure project complies with local codes & building permits. All Plumbing & Electrical provided by customer. Opening must be large enough to receive equipment and area must be level & cleaned for box assembly & equipment. Top of Freezer/Cooler Boxes are not a working platform or to be used for a storage area. DO NOT ACTIVATE POWER to Walk in Door Frame until after the refrigeration system is operational as you can burn out the door wire. It is the owner/operator’s responsibility to secure appropriate protective insurance for reasons outlined in Terms & Conditions –
7. Customer is responsible to advise ABN of any difficulties in access for deliveries and installations as extra charges may incur.
8. ABN Refrigeration assumes no responsibility for product and/or business losses due to delay in installation, malfunction or failure of the equipment, however it is caused.
9. Quote is good for 30 days and payable in Canadian Funds. Delivery for average size box 2 – 3 weeks. Larger boxes & refrigeration requirements may require longer delivery option.

**AMOUNT OF CHEQUE:­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DATE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**